# Brick Wall Instruction

|  |  |  |
| --- | --- | --- |
| **Step 1**  Drill a 25mm hole through the internal brick wall |  | **Step 2**  Drill for 2 seconds into external brick wall to create counter-sunk identification |
| C:\Users\mike\Desktop\cable\Bstep1.jpg |  |  |

|  |  |  |
| --- | --- | --- |
| **Step 3**  Slide Faceplate along keyway until it stops |  | **Step 4**  Drill for 2 seconds into external brick wall to create counter-sunk identification |
|  |  |  |

Brick Wall Instruction Page 2

|  |  |  |
| --- | --- | --- |
| **Step5**  Gently insert band into tool. | | |
|  |  |  |

|  |  |  |
| --- | --- | --- |
| **Step 6**  Drop weighted stringline until its 400mm past the band |  | **Step 7**  Pull Band out capturing stringline |
|  |  |  |

|  |  |  |
| --- | --- | --- |
| **Step 8**  Continue to pull band out to reveal stringline |  | **PRODUCT WARNING** |
|  |  | **Do not use this product near live wires  This product is not a toy please keep out of reach of children  Contains sharp objects and small parts that might be a choking hazard.** |